**STANDARD EQUIPMENT**

Power – assisted steering system

12v DC/240v AC electrical system

220/240v shore power with 35-amp float battery charger

Remote control electric anchor winch

Electro-hydraulic trim tabs

VHF with DSC R/T

Speed and distance log

Echo Sounder with alarm

Remote control with alarm

Remote control searchlight

Combination microwave/ conventional oven grill

Refrigerator with deep freeze compartment

Cockpit wet bar including sink and top loading cool

Box (optional electric barbecue)

Electric quiet flush toilet

Saloon stereo CD/radio/MP3 and cockpit speakers

Teak-laid cockpit and transom platform

Hot and cold transom shower

Tonneau cover

Cockpit sunroof with electric operation

Twin Volvo D6-330DP (2x330 mhp)- Stern drive

Bow thruster

**HULL COLOR**

White

**INTERIOR FURNITURE**

Serotina Cherry wood satin finish (teak galley floor is standard)

Saloon to have timber floor in place of carpet

**LAYOUT**

Sunbed option- aft seat extension with sliding backrest so as to covert to sunbed

**FACILITY**  
Loudspeakers linked to saloon radio fitted in forward coach roof  
  
**NAVIGATION**  
The V39 is fitted with Ray marine i70 color multifunction display (for  
speed, distance, trip, depth, depth alarm, water temperature etc,  
Ray marine e125 Chart plotter/GPS with extemal GPS and 12.1" brilliant  
color multifunction display  
  
Automatic pilot(Ray marine p70R with color display and rate gyro)  
  
**AIRCONDITIONING**  
Air-conditioning, 2 x 12,000btu units (with reverse cycle heating)  
supplying saloon, forward & aft cabins and bathroom  
Rccommended generator: 4Kw  
HOLDING TANK/TOILETS  
  
SYSTEM 2: Toilet discharging into the holding tank but also having the  
ability to discharge directly overboard via a Y valve fitted in the  
Discharge lines. The holding tank has electric overboard discharge as  
well as reserve manual and dockside discharge arrangements  
  
EXTERIOR UPHOLSTERY/CANVAS COVERS  
Foredeck sunbed cushions in white vinyl with contrast paneling to  
upstand of cushions  
Charcoal grey umbrella anti reflective cover to horizontal area behind  
Windscreen(easily removable, located by poppers)  
Black mesh windscreen covers  
Full height cockpit cover in white sunbrella with removable sides and  
Back( on telescopic stainless steel frame& vertical supports) in place of  
Standard tonneau cover top acts as sun awning when sides are removed)

Aft cabin to have sliding double berth conversion  
Heat reflective blind (fitted in place with suction caps) to saloon overhead  
Skylight with storage bag  
**GALLEY**Midnight skype galley top  
COLOR SCHEME  
Additional charge for ultra-leather for saloon sofa  
**DECK HARDWARE**  
Note: the maximum weight allowed for a tender, including outboard, is  
100kg to ensure satisfactory handling and performance)  
Sliding side window at helm position (aperture 36cm H x 38cm L)  
  
Transom platform to have electro-hydraulic lift mechanism  
(Note: The safe working load of the platform is 250kg, but the maximum  
weight of tender and outboard remain at 100kg) raised teak deck at helm position  
  
**GENERATOR**  
Price includes shore support changeover switch and remote control panel  
ONAN 4 Kw/50Hz generator (with hydro hush exhaust system and sound  
shield)  
  
**ELECTRICAL**Continental 220v/240v sockets  
Electric hob (2 burner) in place of standard gas hob and gas  
System  
Electric BBQ in cockpit wet bar  
12v Exterior splash proof power point (cach - specify location)  
Underwater transom lights (2 AMPHIBIAN A6 LED)  
Blue low level cockpit and bathing platform led. Lights  
  
AUDIO VISUAL & COMMUNICATIONS  
Saloon -26" LED TV when this option is requested the standard  
iPod/MP3/Radio is upgraded to FusionIP700 with video &Bluetooth